description[de] = <b>EAGLE Design Rules für Camino v1.3</b>\n<p>\nDie Standard-Design-Rules sind so gewählt, dass sie für \ndie meisten Anwendungen passen. Sollte ihre Platine \nbesondere Anforderungen haben, treffen Sie die erforderlichen\nEinstellungen hier und speichern die Design Rules unter \neinem neuen Namen ab.
description[en] = <b>EAGLE Design Rules</b>\n<p>\nThe default Design Rules have been set to cover\na wide range of applications. Your particular design\nmay have different requirements, so please make the\nnecessary adjustments and save your customized\ndesign rules under a new name.
layerSetup = (1*16)
mtCopper = 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm
mtIsolate = 1.5mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm
mdWireWire = 0.5mm
mdWirePad = 0.5mm
mdWireVia = 0.5mm
mdPadPad = 0.5mm
mdPadVia = 0.5mm
mdViaVia = 0.5mm
mdSmdPad = 0.5mm
mdSmdVia = 0.5mm
mdSmdSmd = 0.5mm
mdViaViaSameLayer = 8mil
mnLayersViaInSmd = 2
mdCopperDimension = 5mm
mdDrill = 8mil
mdSmdStop = 0mil
msWidth = 0.5mm
msDrill = 1mm
msMicroVia = 9.99mm
msBlindViaRatio = 0.500000
rvPadTop = 0.250000
rvPadInner = 0.250000
rvPadBottom = 0.250000
rvViaOuter = 0.500000
rvViaInner = 0.500000
rvMicroViaOuter = 0.250000
rvMicroViaInner = 0.250000
rlMinPadTop = 0.4mm
rlMaxPadTop = 0.8mm
rlMinPadInner = 0.4mm
rlMaxPadInner = 0.8mm
rlMinPadBottom = 0.4mm
rlMaxPadBottom = 0.8mm
rlMinViaOuter = 0.4mm
rlMaxViaOuter = 0.8mm
rlMinViaInner = 0.4mm
rlMaxViaInner = 0.8mm
rlMinMicroViaOuter = 4mil
rlMaxMicroViaOuter = 0.8mm
rlMinMicroViaInner = 4mil
rlMaxMicroViaInner = 0.8mm
psTop = -1
psBottom = -1
psFirst = -1
psElongationLong = 100
psElongationOffset = 100
mvStopFrame = 1.000000
mvCreamFrame = 0.000000
mlMinStopFrame = 4mil
mlMaxStopFrame = 4mil
mlMinCreamFrame = 0mil
mlMaxCreamFrame = 0mil
mlViaStopLimit = 0mil
srRoundness = 0.000000
srMinRoundness = 0mil
srMaxRoundness = 0mil
slThermalIsolate = 0.4mm
slThermalsForVias = 0
dpMaxLengthDifference = 10mm
dpGapFactor = 2.500000
checkGrid = 0
checkAngle = 0
checkFont = 1
checkRestrict = 1
useDiameter = 13
maxErrors = 50
